{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["ZUL ABL Baugruppe","ABL Baugruppe"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ZUL ABL Baugruppe","index":0,"n_rows":42,"n_cols":21,"rows_kept":42,"cut":false,"hidden":false,"merged":[[41,1,41,2],[40,1,40,2],[19,1,19,2],[39,1,39,2],[20,1,20,2]]}
["PROJEKT: "]
[]
[]
[]
["Wohnung","Typ","ZUL","Abluft- und Zulufträume","ANZ Whg","SN100","Summe","ZUL TV100","Summe","ABL TV100","Summe","SN125","Summe","ZUL TV125","Summe","ABL TV125","Summe","Abg.","m/Abg.","Gesamt/Whg","Summe"]
[null,"2-Zimmer","rechts","Bad, WC, Schlafen (Gerät im WZ, 45m3/h)",null,1,{"$f":"F6*E6","v":0},0,{"$f":"H6*E6","v":0},1,{"$f":"J6*E6","v":0},2,{"$f":"L6*E6","v":0},1,{"$f":"N6*E6","v":0},1,{"$f":"P6*E6","v":0},5,8,{"$f":"R6*S6","v":40},{"$f":"T6*E6","v":0}]
[null,"2-Zimmer","links","Bad, WC, Schlafen (Gerät im WZ, 45m3/h)",null,1,0,0,0,1,0,2,0,1,0,1,0,5,8,40,0]
[null,"2-Zimmer","rechts","Bad, WC, Schlafen, Wohnen (Gerät im WZ, 60m3/h)",null,1,0,0,0,1,0,2,0,1,0,1,0,5,8,40,0]
[null,"2-Zimmer","links","Bad, WC, Schlafen, Wohnen (Gerät im WZ, 60m3/h)",null,1,0,0,0,1,0,2,0,1,0,1,0,5,8,40,0]
[null,"2-Zimmer","rechts","Bad, Küche, Schlafen, Wohnen (Gerät im WZ, 60m3/h)",null,0,0,0,0,0,0,3,0,1,0,2,0,6,8,48,0]
[null,"2-Zimmer","links","Bad, Küche, Schlafen, Wohnen (Gerät im WZ, 60m3/h)",null,0,0,0,0,0,0,3,0,1,0,2,0,6,8,48,0]
[null,"3-Zimmer","rechts","Bad, WC, Schlafen, Kind (Gerät im WZ, 60m3/h)",null,2,0,1,0,1,0,2,0,1,0,1,0,6,8,48,0]
[null,"3-Zimmer","links","Bad, WC, Schlafen, Kind (Gerät im WZ, 60m3/h)",null,2,0,1,0,1,0,2,0,1,0,1,0,6,8,48,0]
[null,"3-Zimmer","rechts","Bad, Küche, Schlafen, Kind (Gerät im WZ, 60m3/h)",null,1,0,1,0,0,0,3,0,1,0,2,0,7,8,56,0]
[null,"3-Zimmer","links","Bad, Küche, Schlafen, Kind (Gerät im WZ, 60m3/h)",null,1,0,1,0,0,0,3,0,1,0,2,0,7,8,56,0]
[null,"3-Zimmer","rechts","Bad, Küche, Schlafen, Kind, Wohnen (Gerät im WZ, 60m3/h)",null,1,0,1,0,0,0,3,0,1,0,2,0,7,8,56,0]
[null,"3-Zimmer","links","Bad, Küche, Schlafen, Kind, Wohnen (Gerät im WZ, 60m3/h)",null,1,0,1,0,0,0,3,0,1,0,2,0,7,8,56,0]
[null,null,null,null,{"$f":"SUM(E6:E17)","v":0},null,{"$f":"SUM(G6:G17)","v":0},null,{"$f":"SUM(I6:I17)","v":0},null,{"$f":"SUM(K6:K17)","v":0},null,{"$f":"SUM(M6:M17)","v":0},null,{"$f":"SUM(O6:O17)","v":0},null,{"$f":"SUM(Q6:Q17)","v":0},null,null,null,{"$f":"SUM(U6:U17)","v":0}]
[]
["Stück","Art.-Nr.",null,"Artikel"]
[{"$f":"E18","v":0},"KLL70VT252",null,"ZUL/ABL Verteilereinheit 25cm"]
[{"$f":"E18","v":0},"KLL70BGOR25",null,"Baugruppe Air70 rechts 25cm"]
[{"$f":"E18*2","v":0},"KLLKUNI100",null,"Doppelnippel DN100"]
[{"$f":"ROUNDUP(E18*5.2/25,0)","v":0},"KLLAIRSF20",null,"Bauteilfugenabdichtungsband innen"]
[{"$f":"ROUNDUP(E18*5.2/25,0)","v":0},"KLLAIRSF2",null,"Bauteilfugenabdichtungsband aussen"]
[{"$f":"E18-(E8+E9+E10+E11+E16+E17)","v":0},"KLL70UAD",null,"Abdeckung Glas weiß"]
[{"$f":"E8+E9+E10+E11+E16+E17","v":0},"KLL70UIB",null,"Innenblende Glas weiß (ZUL unten)"]
[{"$f":"E18","v":0},"KLL70FLAAF",null,"Fassadenanschluss AUL/FOL"]
[{"$f":"G18","v":0},"KLLZSN10075",null,"Saugnische 100"]
[{"$f":"M18","v":0},"KLLZSN125752",null,"Saugnische 125"]
[{"$f":"G18","v":0},"KLLZSNFL100",null,"Flansch 100"]
[{"$f":"M18","v":0},"KLLZSNFL125",null,"Flansch 125"]
[{"$f":"I18","v":0},"KLLZZULV100",null,"ZUL-Tellerventil 100"]
[{"$f":"O18","v":0},"KLLZZULV125",null,"ZUL-Tellerventil 125"]
[{"$f":"K18","v":0},"KLLZABLV100",null,"ABL-Tellerventil 100"]
[{"$f":"Q18","v":0},"KLLZABLV125",null,"ABL-Tellerventil 125"]
[{"$f":"E10+E11+E14+E15+E16+E17","v":0},"PKEA75/45",null,"Polokal-T-Stück 45° 75mm"]
[{"$f":"ROUNDUP(U18/5,-1)*5","v":0},"KLLZSCHL75",null,"Kunststoffschlauch 75mm"]
[{"$f":"ROUNDDOWN(A38/51,0)+A37","v":0},"KLLZVEM75",null,"Verbindungsmuffe 75mm"]
[{"$f":"E7+E9+E11+E13+E15+E17","v":0},"KLLZKZ753",null,"3-fach-Kreuzungsstück DN75"]
[{"$f":"E8+E9+E10+E11+E16+E17","v":0},"HOIBN/KL/70W1",null,"Inbetriebnahme "]
[{"$f":"E18-A41","v":0},null,null,"Inbetriebnahme bei Bedarf auf Anfrage"]

{"sheet":"ABL Baugruppe","index":1,"n_rows":28,"n_cols":21,"rows_kept":28,"cut":false,"hidden":false,"merged":[[27,1,27,2],[4,1,4,2],[5,1,5,2],[6,1,6,2],[9,1,9,2],[14,1,14,2],[10,1,10,2]]}
["PROJEKT: "]
[]
[]
[]
["Wohnung","Typ",null,"Abluft- und Zulufträume","ANZ Whg","SN100","Summe","ZUL TV100","Summe","ABL TV100","Summe","SN125","Summe","ZUL V125","Summe","ABL TV125","Summe","Abg.","m/Abg.","Gesamt/Whg","Summe"]
[null,"1-Zimmer",null,"Bad, Schlafen (Gerät im SZ, 45m3/h)",null,0,{"$f":"F6*E6","v":0},0,{"$f":"H6*E6","v":0},0,{"$f":"J6*E6","v":0},1,{"$f":"L6*E6","v":0},0,{"$f":"N6*E6","v":0},1,{"$f":"P6*E6","v":0},2,8,{"$f":"R6*S6","v":16},{"$f":"T6*E6","v":0}]
[null,"1-Zimmer",null,"WC, Bad, Schlafen (Gerät im SZ, 45m3/h)",null,1,0,0,0,1,0,1,0,0,0,1,0,3,8,24,0]
[null,null,null,null,{"$f":"SUM(E6:E7)","v":0},null,{"$f":"SUM(G6:G7)","v":0},null,{"$f":"SUM(I6:I7)","v":0},null,{"$f":"SUM(K6:K7)","v":0},null,{"$f":"SUM(M6:M7)","v":0},null,{"$f":"SUM(O6:O7)","v":0},null,{"$f":"SUM(Q6:Q7)","v":0},null,null,null,{"$f":"SUM(U6:U7)","v":0}]
[]
["Stück","Art.-Nr.",null,"Artikel"]
[{"$f":"E8","v":0},"KLL70VT25",null,"Verteilereinheit 25cm inkl. Ausgleichselement"]
[{"$f":"E8","v":0},"KLL70BG25",null,"Baugruppe Air70 25cm"]
[{"$f":"E8","v":0},"KLLKUNI100",null,"Doppelnippel DN100"]
[{"$f":"ROUNDUP(E8*5.2/25,0)","v":0},"KLLAIRSF20",null,"Bauteilfugenabdichtungsband innen"]
[{"$f":"ROUNDUP(E8*5.2/25,0)","v":0},"KLLAIRSF2",null,"Bauteilfugenabdichtungsband aussen"]
[{"$f":"E8","v":0},"KLL70UIB",null,"Designinnenblende Glas weiß (ZUL unten)"]
[{"$f":"E8","v":0},"KLL70FLAAF",null,"Fassadenanschluss AUL/FOL"]
[{"$f":"G8","v":0},"KLLZSN10075",null,"Saugnische 100"]
[{"$f":"M8","v":0},"KLLZSN125752",null,"Saugnische 125"]
[{"$f":"G8","v":0},"KLLZSNFL100",null,"Flansch 100"]
[{"$f":"M8","v":0},"KLLZSNFL125",null,"Flansch 125"]
[{"$f":"I8","v":0},"KLLZZULV100",null,"ZUL-Tellerventil 100"]
[{"$f":"O8","v":0},"KLLZZULV125",null,"ZUL-Tellerventil 125"]
[{"$f":"K8","v":0},"KLLZABLV100",null,"ABL-Tellerventil 100"]
[{"$f":"Q8","v":0},"KLLZABLV125",null,"ABL-Tellerventil 125"]
[{"$f":"ROUNDUP(U8/5,-1)*5","v":0},"KLLZSCHL75",null,"Kunststoffschlauch 75mm"]
[{"$f":"ROUNDDOWN(A26/51,0)","v":0},"KLLZVEM75",null,"Verbindungsmuffe 75mm"]
[{"$f":"E8","v":0},null,null,"Inbetriebnahme bei Bedarf auf Anfrage"]